|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **REVIEW QUOTATION FOR FABRICATION AND INSTALLATION OF IRON TRUSSES FOR NEW SPRING BAPTIST CHURCH, BAALE YAKU AREA, OGBOMOSO.** | | | | |
| S/N | QTY | MATERIALS SPECIFICATIONS | RATE (N) | AMOUNT (N) | |
| 1 | 164 | lengths of 60x60x6mm for strength trusses | 16,300 | 2673200 | |
| 2 | 60 | lengths of 70x70x6mm for diagonal trusses | 19,000 | 1140000 | |
| 3 | 150 | lengths of 50x50x5mm for bracing and wind brace | 9,500 | 1425000 | |
| 4 | 194 | length of 1.2mm Z-purlin | 10,500 | 2037000 | |
| 5 | 326 | nos of angle cleat | 700 | 228200 | |
| 6 | 80 | lengths of 40x40x4mm cladding angle | 6,000 | 480000 | |
| 7 | 32 | lengths of 25x25x3mm ridge angle | 3,000 | 96000 | |
| 8 | 26 | packets of electrode stone bridge | 5,000 | 130000 | |
| 9 | 30 | gallons of red oxide paint | 7,000 | 210000 | |
| 10 | 8 | dozens of m20 king post bolt & nuts | 5,000 | 40000 | |
| 11 | 300 | litres of diesel fuel | 820 | 246000 | |
| 12 | 6 | bottles of refilled oxyacetylene | 25,000 | 150000 | |
| 13 | 26 | Nos of 300x225x10mm | 4,000 | 104000 | |
| 14 | 104 | Nos of M20 J-Bolts | 1,000 | 104000 | |
| 15 | 1 | Other accessories such as petrol, brush, blade, etc. | 45,000 | 45000 | |
|  |  | **SUB-TOTAL** |  | **9,108,400** | |
|  |  | Transportaion |  | 300,000 | |
|  |  | Workmanship |  | 1,500,000 | |
|  |  | **GRAND TOTAL** |  | **10,908,400** | |